**SP-XX 6” REINFORCED CONCRETE SIDEWALKS (BRIDGING TREE ROOTS, CLDS 40.11)**

Version Date: 08/05/2024 Revision Date: MM/DD/YYYY by XXX

1. **DESCRIPTION**

The work covered by this special provision includes all elements of work covered by section 848, “Concrete Sidewalks, Driveways and Wheel Chair Ramps” of the Standard Specifications. 6” Reinforced Concrete Sidewalk shall be constructed and conform to Charlotte Land Development Standard (CLDS) 40.11 “Bridging Tree Roots”. All methods of installation are to conform with the Charlotte Landscape Constructions Standards Section 01000 Part 03-EXECUTION - L - ROOT PRUNING.

1. **MATERIALS**

All materials shall be in accordance with section 848 of the NCDOT Standard Specifications and CLDS 40.11 Bridging Tree Roots.

1. **MEASUREMENT**

The quantity of 6” Reinforced Concrete Sidewalk to be paid for will be the actual number of square yards of reinforced sidewalk, measured along the surface of the walk that has been constructed and accepted. There will be no separate measurement of, Wooden Forms, #57 Stone, #4 Rebar (reinforcing steel), Rebar Chairs, Groove Joints, Expansion Joints, Expansion Material, Tree Root Cutting, or other work shown on CLDS 40.11.

1. **PAYMENT**

Payment for 6” Reinforced Concrete Sidewalk, as measured above, will be paid for at the contract unit price for “6” Reinforced Concrete Sidewalk (Bridging Tree Roots, CLDS 40.11)” .  There will be no separate payment for, Wooden Forms, #57 Stone, #4 Rebar (reinforcing steel), Groove Joints, Expansion Joints, Expansion Material, Tree Root Cutting or other work shown on CLDS 40.11. Such payment will be full compensation for all work covered by this special provision and includes all labor, equipment, and materials necessary to complete this provision.

Payment will be made under:

**6” REINFORCED CONCRETE SIDEWALK, (BRIDGING TREE ROOTS, CLDS 40.11) SY**